(kicad_pcb
	(version 20250114)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "RF Power and SWR Meter")
		(date "2025-12-05")
		(rev "1.0")
		(company "Open Source Hardware")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "RF_IN")
	(net 3 "RF_OUT")
	(net 4 "FWD_DET")
	(net 5 "REV_DET")
	(footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount"
		(layer "F.Cu")
		(at 30 75 0)
		(descr "SMA RF connector edge mount")
		(tags "SMA connector edge mount")
		(property "Reference" "J1"
			(at 0 -5 0)
			(layer "F.SilkS")
		)
		(property "Value" "RF_IN"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rf-power-swr-meter.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "RF_IN")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3 0)
			(size 2 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3 0)
			(size 2 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount"
		(layer "F.Cu")
		(at 150 75 0)
		(descr "SMA RF connector edge mount")
		(tags "SMA connector edge mount")
		(property "Reference" "J2"
			(at 0 -5 0)
			(layer "F.SilkS")
		)
		(property "Value" "RF_OUT"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rf-power-swr-meter.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "RF_OUT")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3 0)
			(size 2 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3 0)
			(size 2 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 45 75 90)
		(descr "Resistor SMD 0805")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "50"
			(at 0 2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rf-power-swr-meter.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "RF_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 60 75 0)
		(descr "Capacitor SMD 0805")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "10pF"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rf-power-swr-meter.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "FWD_DET")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 60 85 270)
		(descr "SOD-323 Schottky diode")
		(tags "diode schottky")
		(property "Reference" "D1"
			(at 0 -2 270)
			(layer "F.SilkS")
		)
		(property "Value" "1N5711"
			(at 0 2 270)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rf-power-swr-meter.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "FWD_DET")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 90 75 0)
		(descr "Capacitor SMD 0805")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "10pF"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rf-power-swr-meter.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "REV_DET")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 90 85 270)
		(descr "SOD-323 Schottky diode")
		(tags "diode schottky")
		(property "Reference" "D2"
			(at 0 -2 270)
			(layer "F.SilkS")
		)
		(property "Value" "1N5711"
			(at 0 2 270)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rf-power-swr-meter.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "REV_DET")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
	)
	(gr_rect
		(start 20 60)
		(end 160 95)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "RF Power/SWR Meter v1.0"
		(at 90 67 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 20 60) (xy 160 60) (xy 160 95) (xy 20 95)
			)
		)
	)
)
